{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["主机设备"],"read":"whole","date_system":"1900"}

{"sheet":"主机设备","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"merged":[[0,0,0,6]]}
["纺丝设备安装清单"]
["序号","项目名称","单位","数量","所在楼层","装机功率","备注"]
[1,"螺杆挤压机安装找平","台",2,"11m","132+76.2KW","电机132KW，6个加热区共76.2KW"]
[2,"螺杆挤压机基础安装找平","台",2,"11m"]
[3,"熔体夹套管、静态混合器安装、焊接、探伤","套",2,"11m",null,"含保温"]
[4,"计量泵电机支撑架安装找平、焊接","套",2,"11m"]
[5,"计量泵电机及传动轴安装找平","套",8,"11m","4.5KW","规格50cc/r"]
[6,"纺丝箱体托脚安装找平","个",16,"11m"]
[7,"纺丝箱体安装找平","套",2,"11m"]
[8,"纺丝箱洞口封闭","线",2,"11m"]
[9,"组件安装（排料假泵、计量泵，不包括喷丝板的安装）","套",16,"11m"]
[10,"缓冷加热器安装","套",8,"8m","7KW"]
[11,"联苯炉及联苯系统管道安装","套",2,"8m","60KW","包含：管道，阀门、仪表、报检、探伤、保温等"]
[12,"HMLS环吹装置安装找平（包括支吊架）","套",8,"8m"]
[13,"环吹风洞口封闭","线",2,"8m"]
[14,"甬道安装","套",16,"8m"]
[15,"组件装卸机械手安装","套",2,"8m"]
[16,"卷绕基础板找平焊接","套",2,"0m"]
[17,"卷绕机架和导丝器及支架，网络器及支架；热辊及热辊保温箱，油剂油轮上油系统、网络和预网络器托架及外壳、电磁阀和调压阀、内部配管（压空、油雾、油剂、冷却油、排烟），废丝管等","线",2,"0m",null,"2位/线，每个位热辊配置（12个/位）：\nGR1*2(辊壳φ250mm*400mm):驱动11.5+加热12KW\nGR2*2(辊壳φ250mm*400mm):驱动17+加热12KW\nGR3/4/5*2(辊壳φ275mm*400mm):驱动13+加热18KW\nGR6*2(辊壳φ250mm*350mm):驱动8+加热9KW"]
[18,"热辊风冷系统,压空控制单元及过滤器、油雾发生器、油雾分离器、油雾收集站、油冷却单元","线",2,"0m"]
[19,"卷绕头、纺丝卷绕MCC电气配套件、控制电脑、电气辅助柜。","线",2,"0m"]
[]
[null,"注：保温由施工单位包工包料实施。"]